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Quotation No.:	 2309 / OUTR							Dated:  10/07/2026

QUOTATION CALL NOTICE
[bookmark: _Hlk190790389][bookmark: _Hlk218536792]Sealed Quotations are invited from Manufacturers / Registered Firms with OEM/Partners/Agencies/Suppliers having valid PAN/GSTIN/Registration Documents for supply and installation of “Procurement of different items for Power System Lab” for School of Electrical Sciences of the University as per the specifications given below with following terms & condition: -
	Sl no
	Description of item 
	Qty
	Rate per Unit
	GST Rate per Unit 
@__ % 
	Unit Amount with GST
	Total Amount with GST

	1 
	Ring Type Resin Cast LTCT,
CTR:: 5:1, Burden: 5VA, Accuracy Class: 0.5 S Frequency: 50Hz, Single phase, power  3kV,Rated Voltage: 433 Volt.
	03
	
	
	
	

	2 
	Ring Type Resin Cast LT CT, CTR: 10:1,Burden: 5VA,Accuracy Class: 0.5S Frequency:  50Hz, Single phase, power 3kV
	03
	
	
	
	

	3 
	Ring Type Resin Cast LT CT, CTR: 20:1,Burden:5VA,Accuracy Class: 0.5S Frequency: 50Hz,Single phase, power 3kV
	03
	
	
	
	

	4 
	Ring Type Resin Cast LT CT, CTR: 50:1,Burden:5VA,Accuracy Class: 0.5S Frequency: 50Hz, Single phase, power 3kV
	03
	
	
	
	

	5 
	Ring Type Resin Cast LT CT, CTR: 50:5,Burden: 5VA, Accuracy Class: 0.5S Frequency: 50Hz, Single phase, power 3kV
	02
	
	
	
	

	6 
	Ring  Type Resin Cast LT CT, CTR: 100:5, Burden:5VA, Accuracy Class: 0.5S Frequency: 50Hz, Single phase, power 3kV.Rated Voltage : 433 Volt
	02
	
	
	
	

	7 
	Ring Type Wound (Spiral Wound) LT CT, CTR: 5:1,Burden: 5VA,Accuracy Class : 0.5S Frequency: 50Hz,Single phase, power 3kV, Rated Voltage : 433Volt.
	03
	
	
	
	

	8 
	Ring Type Wound (Spiral Wound) LT CT, CTR: 10:1, Burden: 5VA, Accuracy Class : 0.5S Frequency: 50Hz,Single phase, power 3kV, Rated Voltage : 433 Volt.
	03
	
	
	
	

	9 
	Ring Type Wound (Spiral Wound) LT CT, CTR: 20:1, Burden: 5VA, Accuracy Class : 0.5S Frequency: 50Hz,Single phase, power 3kV. Rated Voltage : 433Volt.
	03
	
	
	
	

	10 
	Ring Type Wound (Spiral Wound) LT CT, CTR: 50:5, Burden: 5VA,Accuracy Class : 0.5S Frequency: 50Hz,Single phase, power  3kV
	03
	
	
	
	

	11 
	Ring Type Resin Cast LT CT, CTR:10:1, Burden:15VA, Accuracy Class: 0.5P Frequency: 50Hz, Single phase, power 3kV, ALF: 10
	03
	
	
	
	

	12 
	Ring Type Resin Cast LT CT,
CTR:20:1, Burden:15VA, Accuracy Class: 0.5P Frequency: 50Hz,Single phase, power 3kV, ALF: 10
	03
	
	
	
	

	13 
	Ring Type Resin Cast LT CT,
CTR: 50:1,Burden:15VA,Accuracy Class: 0.5P Frequency: 50Hz,Single phase, power 3kV, 
ALF: 10
	02
	
	
	
	

	14 
	Bar Type Resin Cast LT CT,
CTR: 10:1, Burden:15VA, Accuracy Class: 0.5S Frequency: 50Hz,Single phase, power 3kV.
	03
	
	
	
	

	15 
	Square Type Resin Cast LT  CT,
CTR:10:1, Burden:5VA, Accuracy Class: 0.5S Frequency: 50Hz,Single phase, power 3kV.
	03
	
	
	
	

	16 
	DC Milli Ammeter,0-10-50-100 Ma (Panel Type)
	03
	
	
	
	

	17 
	DC Micro Ammeter, 0-50-100 Micro A (Panel Type)
	02
	
	
	
	

	18 
	Moving Iron Volt Meter,0-150-300V,1Ph 50Hz (Panel Type)
	06
	
	
	
	

	19 
	Moving Iron Ammeter, 0-5-10V, 50Hz
(Panel Type)
	05
	
	
	
	

	20 
	Moving Iron Ammeter,0-10-20V, 50Hz (Panel Type)
	05
	
	
	
	

	21 
	Green Push Button
	10
	
	
	
	

	22 
	Red Push Button
	10
	
	
	
	

	23 
	Single Phase Transformer, 1KVA, 230/40 (Open Type)
	03
	
	
	
	

	24 
	Portable Wooden Case PT440-220-/110V, 15A
	02
	
	
	
	

	25 
	Portable Wooden Case PT660-440-220/110V,15A
	02
	
	
	
	

	26 
	Single Tube Rheostat, 1200 Ohms, 0.6A
	02
	
	
	
	

	27 
	Single Tube Rheostat, 5 Ohms, 2A
	05
	
	
	
	

	28 
	Single Tube Rheostat, 9 Ohms, 12A
	02
	
	
	
	

	29 
	3 Ph 1HP, 415V, DOL Starter
	01
	
	
	
	

	30 
	Auto Transformer 1Ph, 8A
	02
	
	
	
	

	31 
	Auto Transformer 3Ph, 8A
	01
	
	
	
	

	32 
	Power Contactor, 3Phase, 415V, 20A, L&T Make
	02
	
	
	
	

	33 
	Power Contactor, 1Phase, 220V, 20A, L&T Make
	02
	
	
	
	

	34 
	Electric Buzzer,230V
	02
	
	
	
	

	35 
	Time Interval Counter 0-10,000 second
	02
	
	
	
	



Terms and conditions
1. The cost of the above-mentioned item should be quoted mentioning the make, model number and detailed technical specifications.
2. The rate quoted should be inclusive of all packing, delivery and installation.
3. The goods are required to be delivered at this University under the Supplier’s own arrangement without any additional charges. The risk of damage or loss in transit if any will be borne by the supplier.
4. The supplier should super-scribed the quotation as “Procurement of different items for Power System Lab” for School of Electrical Sciences, OUTR, Bhubaneswar in BOLD letters along-with quotation No., due date and time.  
5. The rate quoted must remain valid for 90 days from the date of opening of quotation.
6. Delivery and installation of material should be at OUTR, Bhubaneswar within 30 days from the date of issue of purchase order.
7. It will be the responsibility of the party to provide necessary spare consumables which may be required during the installation at its own cost.
8. The vendors are required to submit the offer along with valid PAN / GSTIN / Registration Certificates.
9. The firm must have not been blacklisted during last three financial years.
10. The warranty should be provided by the vendor for a minimum period of 1 years from the date of delivery and installation.
11. Payment: - Payment will be made by NEFT within 30 days after supply and successful installation of the above item in good condition upon submission of Tax Invoice.
12. Liquidated Damages: In case of delay in supply, the University will recover LD @ 1% of the value of the undelivered goods per month or part thereof subject to a maximum of 5% of the undelivered goods.
13. For any technical query, please contact: - Dr. R. N. Pradhan, 
i. Mob No: 9937113432, 
ii. e-mail: rudranarayan@outr.ac.in


The last date for submission of quotation is 10/08/2026 up to  04:30 PM addressing to the “The Registrar, Odisha University of Technology and Research, Techno Campus, P.O.: Mahalaxmi Vihar, Ghatikia, Bhubaneswar – 751 029” by Speed / Registered Post / Courier only.  Hand delivery is not accepted. The date of opening of bid is 11/08/2026 at  03:00 PM at the HOS, SES Chamber. The authority will not be responsible for any postal delay.  The quotation will not be considered after scheduled date and time. The authority reserves the right to reject any or all quotations without assigning any reason thereof.



												Sd/-
REGISTRAR
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